

|  |  |
| --- | --- |
| Instrument: | Name:  E-mail: |
| **Common specifications** | |
| Model Ennea Bass Doublecut / Ennea Bass Singlecut |  |
| Number of strings 4 / 5 / 6 |  |
| Scale length 34'' / 35'' Multiscale: 4str - 34-35", 5str - 34-36, 6str - 33.5-36" |  |
| Left handed / right handed |  |
| **Neck specifications** | |
| Number of frets 26 |  |
| Fret wire Material - Nickel-silver, Stainless Steel, Evo Gold  Size - only 2.54х1.3mm |  |
| Neck lamination |  |
| Neck wood see the price list |  |
| Fretboard wood see the price list |  |
| Fretboard radius 12” 14'' 16'' 20'' 37'' |  |
| Neck thickness and profile  Thickness 19-22mm /20-23mm/ 21-24mm / Profile ‘’C’’ / ‘’U’’ |  |
| Fretboard binding see the price list |  |
| Fret position markers or custom inlay see the price list |  |
| Side markers see the price list |  |
| Nut see the price list |  |
| Headstock color / veneer / finish see the price list |  |
| Neck color / finish see the price list |  |
| Notes |  |
| **Body specifications** | |
| Body wood see the price list |  |
| Chambering Weight reducing chambers (only with a top) |  |
| Top material see the price list |  |
| Body color / finish see the price list |  |
| Cavity cover material / plastic / wood  Cavity cover mount screws, bolts, magnets |  |
| Notes |  |
| **Hardware / electronics** | |
| Bridge Padalka Hardware / Hipshot Triple Lockdown |  |
| String spacing at the bridge |  |
| Tuners Hipshot Ultralite |  |
| Hardware colour chrome / black / gold |  |
| Pickups |  |
| Pre-amp |  |
| Knob configuration in addition to preamp or with passive electronics |  |
| Pickup selector type mini toggle, rotary switch or balance pot |  |
| Knobs Gotoh Dome-style / Hipshot O-ring / Custom knobs |  |
| Strap buttons Gotoh strap pin or Schaller straplocks |  |
| Strings gauge / Tuning |  |
| Notes |  |
| **Additional information** | |
| Shipping address |  |
| Packing Gig-bag + shipping box / hardshell case |  |
| Notes |  |