

|  |  |
| --- | --- |
| Instrument: | Name:  E-mail: |
| **Common specifications** | |
| Model Neptune / Saturn |  |
| Scale length 25,5'' / 26,5'' / 27'' / 28'' / Multiscale |  |
| Number of strings 6 / 7 / 8 |  |
| Neck joint Bolt on (choose the type of bolts/screws) / set in |  |
| Left handed / right handed |  |
| **Neck specifications** | |
| Number of frets 24 |  |
| Fret wire  Nickel-silver - 2.28х1.4mm / 2.54х1.3mm / 2.79х1.45mm  Stainless Steel - 2.28х1.4mm / 2.54х1.3mm / 2.79х1.45mm  Evo Gold 2.28х1.4mm / 2.79х1.45mm |  |
| Neck pieces 1 / 3 / 5 / 7 |  |
| Neck wood see the price list |  |
| Fretboard wood see the price list |  |
| Fretboard radius 12” 14'' 16'' 20'' 37'' Compound radius |  |
| Neck thickness and profile  Thickness 18-20mm /19-21mm/ 20-22mm / Profile ‘’C’’ / ‘’U’’ |  |
| Headstock end straight / wave |  |
| Fretboard binding 1 or 2 ply / wood or plastic |  |
| Fret position markers MOP or wood dots (2, 4, 6 mm) /  wooden blocks / aluminium rings |  |
| Side markers dots: MOP / plastic / wood / aluminium / luminlay |  |
| Custom inlay |  |
| Nut  Graphite (Japan) / Graphtech (Canada) /Hipshot Zero Friction / Bone |  |
| Headstock colour / veneer / finish  Satin lacquer / Gloss lacquer / Oil (transparent only) |  |
| Neck colour / finish  Satin lacquer / Gloss lacquer / Oil (transparent only) |  |
| Reinforcement Standard (12-24 fret) / full length |  |
| Truss rod One way + spoke wheel / two way  For multiscale instruments - only two way |  |
| Notes |  |
| **Body specifications** | |
| Body wood see the price list |  |
| Chambering Weight reducing chambers (only with top) |  |
| Top material see the price list |  |
| Body colour / finish  Satin lacquer / Gloss lacquer / Oil (only transparent) |  |
| Top colour / finish  Satin lacquer / Gloss lacquer / Oil (only transparent) |  |
| Cavity cover material / plastic / wood  Cavity cover mount screws, bolts, magnets |  |
| Notes |  |
| **Hardware / electronics** | |
| Tuners / Bridge Hipshot Headless System / Mera Submarine |  |
| Hardware colour chrome / black / gold |  |
| Strings gauge / Tuning |  |
| Jack plate only angled barrel jack |  |
| Knobs Gotoh Dome-style / Hipshot O-ring |  |
| Pickups |  |
| Knob configuration  volume, tone, 3/5-way switch.+ wiring option (see diagram) |  |
| Split coils none / pickup switch / push-pull / mini toggle |  |
| Pickup selector type for 3-way switch - blade or toggle |  |
| Strap buttons Gotoh strap pin or Schaller straplocks |  |
| Notes |  |
| **Additional information** | |
| Shipping address |  |
| Shipment packing / hardshell case / guitar strap |  |
| Notes |  |