

|  |  |
| --- | --- |
| Instrument:  | Name:E-mail: |
| **Common specifications** |
| Model Space / Moon / CS / Mars |  |
| Scale length 24,75'' / 25,5'' / 26,5'' / 27'' / 28'' / Multiscale |  |
| Number of strings 6 / 7 / 8 |  |
| Neck joint Bolt on (choose the type of bolts/screws) /  set in / neck through (only for Moon and CS) |  |
| Left handed / right handed  |  |
| **Neck specifications** |
|  Number of frets 24 |  |
|  Fret wireNickel-silver - 2.28х1.4mm / 2.54х1.3mm / 2.79х1.45mmStainless Steel - 2.28х1.4mm / 2.54х1.3mm / 2.79х1.45mmEvo Gold 2.28х1.4mm / 2.79х1.45mm |  |
|  Neck pieces 1 / 3 / 5 / 7 |  |
|  Neck wood see the price list |  |
|  Fretboard wood see the price list |  |
|  Fretboard radius 12” 14'' 16'' 20'' 37'' Compound radius |  |
|  Neck thickness and profile Thickness 18-20mm /19-21mm/ 20-22mm / Profile ‘’C’’ / ‘’U’’ |  |
| Headstock shape A-1 / A-2 / A-3 / CS / MS |  |
| Binding: fretboard / headstock 1 or 2 ply  Fretboard – wood or plastic / headstock – plastic or scraped  |  |
| Fret position markers MOP or wood dots (2, 4, 6 mm) / wooden blocks / aluminium rings |  |
| Side markers dots: MOP / plastic / wood / aluminium / luminlay |  |
| Custom inlay |  |
| Nut Graphite (Japan) / Graphtech (Canada) / Hipshot Zero Friction / Bone / Roller nut (6str) |  |
| Headstock colour / veneer / finish Satin lacquer / Gloss lacquer / Oil (transparent only) |  |
| Neck colour / finish Satin lacquer / Gloss lacquer / Oil (transparent only) |  |
| Reinforcement Standard (12-24 fret) / full length |  |
| Notes |  |
| **Body specifications** |
| Body wood see price |  |
| Arm bevel (for CS, Mars, Space) / chamfer (for Moon) / carved top (for CS and Space)  |  |
| Chambering Weight reducing chambers (only with top) |  |
| Top material see the price list |  |
| Body binding 1 or 2 ply / plastic or scraped |  |
| Body colour / finish Satin lacquer / Gloss lacquer / Oil (only transparent) |  |
| Top colour / finish Satin lacquer / Gloss lacquer / Oil (only transparent) |  |
| Cavity cover material / plastic / woodCavity cover mount screws, bolts, magnets  |  |
| Notes |  |
| **Hardware / electronics** |
| Bridge Hipshot Hardtail / Schaller Tremolo / Floyd Rose |  |
| Tuners Hipshot Griplock (locking) / Gotoh SG381 (non locking) |  |
| Hardware colour chrome / black / gold |  |
| Strings gauge / Tuning |  |
| Jack plate Space – barrel jack/ Moon, Mars, CS – oval jack plate |  |
| Knobs Gotoh Dome-style / Hipshot O-ring |  |
| Truss rod cover cover / no cover , wood / plastic |  |
| Pickups |  |
| Pickups mount: rings / direct |  |
| Knob configuration volume, tone, 3/5-way switch.+ wiring option (see diagram) |  |
| Split coils none / pickup switch / push-pull / mini toggle |  |
| Pickup selector type for 3-way switch - blade or toggle |  |
| Pre-amp / piezo saddles Graphtech Ghost |  |
| Strap buttons Gotoh strap pin or Schaller straplocks |  |
| Notes |  |
| **Additional information** |
| Shipping address |  |
| Shipment packing / hardshell case / guitar strap  |  |
| Notes |  |